# CYW954591 WLBGA iPA, iLNA board for bringup -
NVRAMRev=$Rev$
cckdigfilttype=4
#valid ofdm filter types are 0 and 1
ofdmfilttype_2gbe=127
ofdmfilttype_5gbe=127
sromrev=11
boardrev=0x1106
boardtype=0x0863
# JIRA:SW4349-945 MANDATORY! Update makefile in case you touch bfl
# Two Range TSSI boardflag setting and LTE COEX
boardflags=0x00480201
boardflags2=0x00800000
boardflags3=0x48700186
wlbga5g80=1
opt_89359B1=1
macaddr=00:90:4c:31:10:e2
ccode=0
regrev=0
antswitch=0
pdgain5g=0
pdgain2g=0
# Two Range TSSI enable
tworangetssi2g=0
tworangetssi5g=0
# Low power range TSSI cal enable
lowpowerrange2g=0
lowpowerrange5g=0
# Low Power Range start value: 0dBm
#olpc_thresh2g=1
#olpc_thresh5g=0
# Power detector parameters
AvVmid_c0=2,130,2,130,2,130,2,130,2,130
AvVmid_c1=2,130,2,130,2,130,2,130,2,130
# JIRA:SW4349-945 MANDATORY! Update makefile in case you touch femctl
#femctrl=14
vendid=0x14e4
# Spectrum mask parameter
# 0: disabled /  1: mild shaping  /  2: moderate shaping  / 3: strong shaping  /  4: optimized for BCM4359
fdss_level_2g=5,5
fdss_level_5g=4,4
fdss_interp_en=1
#papd_optf=1
#devid not been used now
devid=0x4417
manfid=0x2d0
#prodid=0x052e
nocrc=1
sco_rssi_thresh=-75
otpimagesize=502
xtalfreq=37400
rxgains2gelnagaina0=0
rxgains2gtrisoa0=15
rxgains2gtrelnabypa0=0
rxgains5gelnagaina0=0
rxgains5gtrisoa0=7
rxgains5gtrelnabypa0=0
rxgains5gmelnagaina0=0
rxgains5gmtrisoa0=7
rxgains5gmtrelnabypa0=0
rxgains5ghelnagaina0=0
rxgains5ghtrisoa0=7
rxgains5ghtrelnabypa0=0
rxgains2gelnagaina1=0
rxgains2gtrisoa1=15
rxgains2gtrelnabypa1=0
rxgains5gelnagaina1=0
rxgains5gtrisoa1=7
rxgains5gtrelnabypa1=0
rxgains5gmelnagaina1=0
rxgains5gmtrisoa1=7
rxgains5gmtrelnabypa1=0
rxgains5ghelnagaina1=0
rxgains5ghtrisoa1=7
rxgains5ghtrelnabypa1=0
rrcalphasel=1
rxchain=3
txchain=3
aa2g=3
aa5g=3
agbg0=2
agbg1=2
aga0=2
aga1=2
tssipos2g=1
extpagain2g=2
tssipos5g=1
extpagain5g=2
tempthresh=110
tempoffset=255
rawtempsense=35

#pa2gccka0=0xFF53,0x20A0,0xFC20
pa2gccka0=-213,6753,-835
#pa2gccka1=0xFF43,0x1F5E,0xFC39
pa2gccka1=-209,6682,-832
#pa2ga0=0xFF42,0x1B8E,0xFCBD
pa2ga0=-196,6595,-798
#pa2ga1=0xFF39,0x1B4F,0xFCBE
pa2ga1=-178,7430,-881
#pa5gbw4080a0=0xFF38,0x1E02,0xFC51,0xFF3B,0x1E65,0xFC44,0xFF3E,0x1DB4,0xFC61,0xFF33,0x1B95,0xFC98
pa5gbw4080a0=-375,3770,-684,-323,4507,-718,-402,3220,-636,-292,5536,-825
#pa5gbw4080a1=0xFF2B,0x1CD2,0xFC6E,0xFF29,0x1C1F,0xFC82,0xFF2E,0x1BC4,0xFC93,0xFF28,0x1A89,0xFCB6
pa5gbw4080a1=-228,6427,-844,-203,6705,-872,-192,7104,-884,-364,4254,-750
##V4
#pa5ga0=0xFF31,0x1BB3,0xFC9F,0xFF30,0x1BCD,0xFC9B,0xFF33,0x1BF6,0xFC95,0xFF33,0x1BF6,0xFC95
#pa5ga1=0xFF2A,0x1B15,0xFCAA,0xFF3A,0x1D50,0xFC73,0xFF2D,0x1BA4,0xFC99,0xFF25,0x1924,0xFCE3
##V5, X1 band CORE1 shift down 0.5dB
#pa5ga0=0xFF31,0x1AFF,0xFCB1,0xFF30,0x1ACD,0xFCB5,0xFF33,0x1B69,0xFCA3,0xFF33,0x1AB6,0xFCB5
pa5ga0=-119,8375,-990,-153,7648,-924,-158,6739,-838,-168,7127,-856
#pa5ga1=0xFF2A,0x1AE1,0xFCB0,0xFF3A,0x1C83,0xFC87,0xFF2D,0x1B24,0xFCA6,0xFF25,0x1957,0xFCDF
pa5ga1=-178,7765,-931,-184,7213,-884,-135,8533,-965,-180,7102,-862


maxp2ga0=76
maxp2ga1=76
maxp5ga0=74,74,74,74
maxp5ga1=74,74,74,74
subband5gver=0x4
paparambwver=3
cckpwroffset0=0
cckpwroffset1=1
pdoffset80ma0=0xEEEE
pdoffset80ma1=0xEEEE
cckbw202gpo=0
cckbw20ul2gpo=0
mcsbw202gpo=0x99665533
mcsbw402gpo=0x99665533
dot11agofdmhrbw202gpo=0x6622
ofdmlrbw202gpo=0x0000
mcsbw205glpo=0x97643331
mcsbw405glpo=0x97655551
mcsbw805glpo=0x97655553
mcsbw1605glpo=0
mcsbw205gmpo=0x97643331
mcsbw405gmpo=0x99865551
mcsbw805gmpo=0xc9865553
mcsbw1605gmpo=0
mcsbw205ghpo=0xd8643331
mcsbw405ghpo=0x99865551
mcsbw805ghpo=0xc9865553
mcsbw1605ghpo=0
mcslr5glpo=0x0000
mcslr5gmpo=0x0000
mcslr5ghpo=0x0000
sb20in40hrpo=0x0
sb20in80and160hr5glpo=0x0
sb40and80hr5glpo=0x0
sb20in80and160hr5gmpo=0x0
sb40and80hr5gmpo=0x0
sb20in80and160hr5ghpo=0x0
sb40and80hr5ghpo=0x0
sb20in40lrpo=0x0
sb20in80and160lr5glpo=0x0
sb40and80lr5glpo=0x0
sb20in80and160lr5gmpo=0x0
sb40and80lr5gmpo=0x0
sb20in80and160lr5ghpo=0x0
sb40and80lr5ghpo=0x0
dot11agduphrpo=0x0
dot11agduplrpo=0x0
phycal_tempdelta=15
temps_period=15
temps_hysteresis=5
ltecxmux=0
ltecxpadnum=0x0504
ltecxfnsel=0x44
ltecxgcigpio=0x04
#OOB params
#device_wake_opt=1
#host_wake_opt=0
swctrlmap_2g=0x00001000,0x00000808,0x10081008,0x060000,0x1f9
swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x003
swctrlmap_5g=0x00002000,0x00000040,0x20002000,0x000000,0x1f9
swctrlmapext_5g=0x00000001,0x00000000,0x00010001,0x000000,0x003
fem_table_init_val=0x00001008,0x00002000
fem_table_init_val_ext=0x00000000,0x00000001
rssi_delta_2g_c0=0,0,0,0
rssi_delta_2g_c1=-1,0,-1,0
rssi_delta_5gl_c0=-1,2,-2,2,0,0
rssi_delta_5gl_c1=0,2,-2,2,1,1
rssi_delta_5gml_c0=-1,2,-2,2,-2,5
rssi_delta_5gmu_c0=-2,2,-3,2,0,5
rssi_delta_5gh_c0=-2,-2,-3,0,0,2
rssi_delta_5gh_c1=-1,1,-2,0,0,1
rssi_delta_5gml_c1=-1,1,-2,2,-2,3
rssi_delta_5gmu_c1=-1,1,-2,2,0,3
fuart_pup_rx_cts=1
seci_uart_gpios=0x08090a0b
module_type=0x0
muxenab=1
adjpaldo=0x4

#power per rate back off at high temperature
ppr_hitemp_offset=75
cckbw202gpo_ht=0x3344
ofdmbw202gpo_ht=0x24567777
mcsbw202gpo_ht=0x33666677
ofdmbw205gpo_ht=0x11122222
mcsbw205gpo_ht=0x55222222
mcsbw405gpo_ht=0x65444444
mcsbw805gpo_ht=0x66642211


#avs_enab=1

# 11b CDD mode
# 0: enabled  /  1: disabled, Antenna diversity
cck_onecore_tx=1

# BTC setting
btcdyn_flags=3
btcdyn_dflt_dsns_level=0
btcdyn_low_dsns_level=0
btcdyn_mid_dsns_level=14
btcdyn_high_dsns_level=11
btcdyn_default_btc_mode=4
btcdyn_dsns_rows=4
btcdyn_dsns_row0=4,8,0,-61,-67
btcdyn_dsns_row1=4,0,0,-65,-67
btcdyn_dsns_row2=5,4,0,-63,-67
btcdyn_dsns_row3=5,0,0,-65,-67
btc_mode=4


powoffstemprange=0,70
powoffs2gtla0=-2,-2,-2,-2,-1,-1,-1,-1,-2,-2,-2,-2,-3,-3
powoffs2gtla1=-3,-3,-3,-3,-3,-3,-3,-2,-2,-2,-1,-1,-1,-1
powoffs2gtna0=0,0,0,0,0,0,0,0,0,0,0,0,0,0
powoffs2gtna1=0,0,0,0,0,0,0,0,0,0,0,0,0,0
powoffs2gtha0=2,2,2,2,2,2,2,2,2,1,1,1,1,1
powoffs2gtha1=2,2,2,2,1,1,1,1,1,1,1,1,0,0

powoffstemprange5g=0,70
powoffs5gtla0=0x2121
powoffs5gtla1=0x2211
powoffs5gtna0=0x0000
powoffs5gtna1=0x0000
powoffs5gtha0=0xfeff
powoffs5gtha1=0xefff

ed_thresh2g=-63
ed_thresh5g=-63

##### eps_offset #########
eps_shift0=-2,-2,-3,-1,-2,-3,-1,-1
eps_shift1=-2,-2,-2,-2,-2,-2,-1,-1
eps_shift2=-1,-1,-1,-1,-1,-1

## FCC power limit on ch12/13  FCC power limit in quarter dB
#fccpwrch12=40
#fccpwrch13=1
#fccpwroverride=0
#desense_mode=7	no corresponding code at DINGO & IGUANA
#bphy_predet_en=2 no corresponding code at DINGO & IGUANA
